Decentral window rebate vent for uPVC windows with exclusively automatic flow rate control through control flaps and installation in the upper sash regardless of window hardware. Concealed installation in the window rebate, without milling. Installation by locking into the groove of the sash overlap gasket. Vent is invisible when the window is closed. There are no elements that need to be operated and no visible vent elements attached additionally.

Exchange gaskets (included in delivery) allow the air to enter respectively exit in the area of the external frame gasket.

**The following certificates issued by notified testing bodies must be presented:**

* air permeability including air flow rate characteristic curve according to DIN EN 13141-1
* watertightness according to DIN EN 12208 in association with DIN EN 1027
* sound reduction value Rw according to EN ISO 10140-2, assessed according to EN ISO 717-1

product to offer: arimeo classic S

gasket colour of the window: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

quantity: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

unit: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

unit price: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

total price: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_